Gowning for Entry to the Assembly Cleanroom
EXAMPLE for a fictional company. Every spec value is an example value, not a recommendation. Replace it with the value from your drawing, specification or qualified procedure.
From coplain.com/blog/cleanroom-gowning-work-instruction-example: how to adapt it and common mistakes are on that page.
Document control
	Document no.
	WI-CR-002 (example)

	Revision
	E

	Applies to
	Everyone entering the assembly cleanroom: operators, maintenance, visitors

	Owner
	Cleanroom supervisor

	Approved by
	Quality manager (signature on master copy)

	Training
	Gowning qualification recorded on the skills matrix before unescorted entry


Tools, materials and PPE
1. Locker for personal items
1. Hand-washing sink with soap and paper towels; hand sanitizer
1. Hair cover, beard cover where needed, face mask
1. Cleanroom hood, coverall and boots in the correct size
1. Safety glasses or goggles
1. Cleanroom gloves; 70% isopropyl alcohol spray for gloves (example value)
1. Full-length mirror
Steps
	No.
	Step
	Key point
	Reason

	1
	Prepare before the gowning room. Remove jewelry, watches and phones and put them in your locker with outerwear. Remove makeup. Report any illness, rash or sunburn to the supervisor.
	Nothing goes into the cleanroom that is not on the approved list.
	Jewelry and cosmetics shed particles and can tear gloves or garments; illness raises shedding.

	2
	Wash your hands. Wash hands and forearms with soap for at least 20 seconds (example value), rinse, and dry with a paper towel.
	Turn off the tap with the towel, not your clean hand.
	Clean hands carry fewer particles and microorganisms onto the garments you are about to handle.

	3
	Cover hair and face. Put on the hair cover so all hair is inside, then a beard cover if you have facial hair, then the face mask.
	No hair visible at the forehead, ears or neck. Mask over the nose.
	Covering the head first stops hair and skin falling onto the coverall as you put it on.

	4
	Put on the hood. Take the hood from its pack touching only the inside. Put it on and fasten it so it covers the hair cover, ears and neck.
	Handle garments by the inside wherever possible.
	The outside of the garment faces the room and must stay clean.

	5
	Put on the coverall. Unfold the coverall without letting it touch the floor. Step in one leg at a time, pull it up, put your arms in, tuck the hood skirt inside the collar and zip up.
	If any part of the coverall touches the floor, discard it and take a new one.
SAFETY: Sit or hold the rail while stepping into the legs to keep your balance.
	The floor on the less clean side of the gowning room is the dirtiest surface in the area.

	6
	Put on boots across the bench. Sit on the step-over bench. Put on one boot, tuck the coverall leg inside, fasten it and swing that leg over to the clean side. Repeat with the other leg.
	A booted foot only ever touches the clean side.
SAFETY: Swing your legs over slowly and keep a hand on the bench. Gowning room floors can be slippery.
	The bench is the line between less clean and clean; crossing it with an unbooted foot carries dirt across.

	7
	Put on eye protection and gloves. Put on safety glasses or goggles. Sanitize your hands, then put on gloves, pulling each cuff over the coverall sleeve.
	Glove cuffs over the sleeves, no gap at the wrist. Change any glove that tears.
	Gloves go on last so they cover hands that touched everything else.

	8
	Sanitize gloves and check in the mirror. Spray gloves with the alcohol and let them dry. Check yourself in the full-length mirror front and back.
	No skin or hair showing except around the eyes; all fasteners closed; no tears.
SAFETY: Isopropyl alcohol is flammable. No ignition sources in the gowning room, and let gloves dry before touching anything electrical.
	A mirror check catches gaps you cannot feel.

	9
	Enter and record. Enter through the airlock, letting one door close before opening the next. Sign the entry log.
	Never hold both airlock doors open.
	The airlock keeps the pressure difference that stops less clean air flowing in.


Acceptance criteria
1. All garments in the correct order and size, none touched the floor or the less clean side.
1. No skin or hair visible except around the eyes.
1. Glove cuffs over coverall sleeves, gloves sanitized and dry.
1. Mirror check done front and back with no tears or open fasteners.
1. Entry recorded in the cleanroom log.
Sign-off
	Prepared by
	
	Date
	

	Approved by
	
	Date
	

	Trained / signed by operator
	
	Date
	


